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Figure 4a
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Figure 5b
Stereogram of fault surface with markings of siliceous gouge: bruised step (BS), accretion spall (AS),

gouge "smearing out” (GS) in the direction of movement, pluck step (PS).
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Step-like asperities facing into
direction whence the opposite
fault surface originated
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